**New Thickness:**

mm

mm

5.1

**WAIT**

**Beam Degrader GUI**

**Sheet Thickness**

**Enter**

**Previous Thickness:**

**12.80 mm :**

**0.40 mm :**

**0.80 mm :**

**Actuator Status**

**Reset all Actuators:**

**RESET**

**Status:**

**Power:**

1.5

**Error**

Completely retracted

In progress

**1.60 mm :**

Completely extended

**0.20 mm :**

**0.10 mm :**

**6.40 mm :**

**3.20 mm :**

Completely extended

Completely retracted

Completely extended

Completely retracted

Completely retracted