**ERROR**

**Beam Degrader GUI**

**Power:**

**Sheet Thickness**

**WAIT**

**Status:**

**RESET**

**Reset all Actuators:**

**Total Air gap Thickness: 2.26 mm**

**0.80 mm :**

**1.60 mm :**

**12.80 mm :**

**0.20 mm :**

**6.40 mm :**

**New Thickness:**

mm

mm

5.1

**Enter**

**Previous Thickness:**

1.5

Completely extended

In progress

Completely retracted

Completely extended

Completely extended

Completely retracted

Completely retracted

Air gap 2: 0.20 mm

Completely retracted

Air gap 4: 0.53 mm5 mm

**3.20 mm :**

Air gap 5: 0.43 mm5 mm

Air gap 4: 0.53 mm5 mm

Air gap 3: 0.53 mm5 mm

**0.40 mm :**

Air gap 2: 0.20 mm

Air gap 1: 0.30 mm

**0.10 mm :**

**Actuator Status**